Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- acquisition_units : tecella_hw_props_ex_01

### - b -

- bessel_value_max : tecella_hw_props
- bessel_value_min : tecella_hw_props
- bits_per_sample : tecella_hw_props
- board_index : tecella_system_monitor_result
- board_result_index : tecella_system_monitor_result

### - c -

- can_be_disabled : tecella_reg_props

### - d -

- description : tecella_lib_props
- device_name : tecella_hw_props
- digital_out : tecella_stimulus_segment_ex
- duration : tecella_stimulus_segment , tecella_stimulus_segment_ex
- duration_delta : tecella_stimulus_segment , tecella_stimulus_segment_ex
- dynamic_system_monitor_count : tecella_hw_props_ex_01

### - h -

- hpf_value_max : tecella_hw_props_ex_01
- hpf_value_min : tecella_hw_props_ex_01
- hw_model : tecella_hw_props
- hwvers : tecella_hw_props

### - l -

- label : tecella_reg_props , tecella_system_monitor_result

### - m -

- max_stimulus_segments : tecella_hw_props

### - n -

- n_utility_dacs : tecella_hw_props
- nchans : tecella_hw_props
- ncslows : tecella_hw_props
- ngains : tecella_hw_props
- nslots : tecella_hw_props
- nsources : tecella_hw_props
- nstimuli : tecella_hw_props

### - p -

- pct_lsb : tecella_reg_props

### - r -

- ramp_steps : tecella_stimulus_segment , tecella_stimulus_segment_ex
- reserved_00 : tecella_hw_props
- reserved_01 : tecella_hw_props
- reserved_02 : tecella_hw_props
- reserved_03 : tecella_hw_props

### - s -

- sample_period_lsb : tecella_hw_props
- sample_period_max : tecella_hw_props
- sample_period_min : tecella_hw_props
- serial_number : tecella_hw_props
- slew : tecella_stimulus_segment_ex
- slew_count : tecella_hw_props_ex_01
- stimulus_delta_count_max : tecella_hw_props
- stimulus_ramp_step_size : tecella_hw_props
- stimulus_ramp_step_size_max : tecella_hw_props_ex_01
- stimulus_ramp_step_size_min : tecella_hw_props_ex_01
- stimulus_ramp_steps_max : tecella_hw_props
- stimulus_repeat_count_max : tecella_hw_props
- stimulus_segment_duration_lsb : tecella_hw_props
- stimulus_segment_duration_max : tecella_hw_props
- stimulus_steering_can_be_disabled : tecella_hw_props_ex_01
- stimulus_steering_index_max : tecella_hw_props_ex_01
- stimulus_steering_index_min : tecella_hw_props_ex_01
- stimulus_units : tecella_hw_props_ex_01
- stimulus_value_lsb : tecella_hw_props
- stimulus_value_max : tecella_hw_props
- stimulus_value_min : tecella_hw_props
- supported : tecella_reg_props
- supports_async_stimulus : tecella_hw_props
- supports_bessel : tecella_hw_props
- supports_chan_set_stimulus : tecella_hw_props_ex_01
- supports_hpf : tecella_hw_props_ex_01
- supports_iclamp_enable : tecella_hw_props_ex_01
- supports_icmd : tecella_hw_props
- supports_oscope : tecella_hw_props
- supports_stimulus_steering : tecella_hw_props_ex_01
- supports_vcmd : tecella_hw_props
- supports_zap : tecella_hw_props

### - t -

- trigger_in_delay_lsb : tecella_hw_props_ex_01
- trigger_in_delay_max : tecella_hw_props_ex_01
- trigger_in_delay_min : tecella_hw_props_ex_01
- type : tecella_stimulus_segment , tecella_stimulus_segment_ex

### - u -

- units : tecella_reg_props , tecella_system_monitor_result
- user_config_count : tecella_hw_props
- user_config_name : tecella_hw_props
- utility_dac_lsb : tecella_hw_props
- utility_dac_max : tecella_hw_props
- utility_dac_min : tecella_hw_props

### - v -

- v_default : tecella_reg_props
- v_divisions : tecella_reg_props
- v_dot : tecella_lib_props
- v_lsb : tecella_reg_props
- v_maj : tecella_lib_props
- v_max : tecella_reg_props
- v_min : tecella_reg_props , tecella_lib_props
- value : tecella_stimulus_segment_ex , tecella_system_monitor_result , tecella_stimulus_segment
- value_delta : tecella_stimulus_segment_ex , tecella_stimulus_segment
- value_expected : tecella_system_monitor_result
- value_expected_max : tecella_system_monitor_result
- value_expected_min : tecella_system_monitor_result

### - z -

- zap_value_lsb : tecella_hw_props
- zap_value_max : tecella_hw_props
- zap_value_min : tecella_hw_props